|  |  |
| --- | --- |
| Equipment description |  |
| Serial No. / or ID |  |
| Manufacturer |  |
| Is calibration necessary to ensure product quality | Y / N if yes, state required frequency of calibration |
| Is training critical to product quality? | Y / N if yes, ensure all users have training recorded on C8 |

|  |  |
| --- | --- |
| Equipment description |  |
| Serial No. / or ID |  |
| Manufacturer |  |
| Is calibration necessary to ensure product quality | Y / N if yes, state required frequency of calibration |
| Is training critical to product quality? | Y / N if yes, ensure all users have training recorded on C8 |

|  |  |
| --- | --- |
| Equipment description |  |
| Serial No. / or ID |  |
| Manufacturer |  |
| Is calibration necessary to ensure product quality | Y / N if yes, state required frequency of calibration |
| Is training critical to product quality? | Y / N if yes, ensure all users have training recorded on C8 |

|  |  |
| --- | --- |
| Equipment description |  |
| Serial No. / or ID |  |
| Manufacturer |  |
| Is calibration necessary to ensure product quality | Y / N if yes, state required frequency of calibration |
| Is training critical to product quality? | Y / N if yes, ensure all users have training recorded on C8 |

|  |  |
| --- | --- |
| Equipment description |  |
| Serial No. / or ID |  |
| Manufacturer |  |
| Is calibration necessary to ensure product quality | Y / N if yes, state required frequency of calibration |
| Is training critical to product quality? | Y / N if yes, ensure all users have training recorded on C8 |